ENVI
description = {
../gdrivers/data/envi_rgbsmall_bsq.img}
samples = 50
lines   = 49
bands   = 3
header offset = 0
file type = ENVI Standard
data type = 1
interleave = bsq
byte order = 0
map info = {Geographic Lat/Lon, 1, 1, -44.84032, -22.932584, 0.003432, 0.003432,WGS-84}
coordinate system string = {GEOGCS["GCS_WGS_1984",DATUM["D_WGS_1984",SPHEROID["WGS_1984",6378137.0,298.257223563]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433]]}
band names = {
Band 1,
Band 2,
Band 3}
