oscilikts
Prev | Orchestra Opcodes and Operators | Next

## oscilikts

oscilikts — A linearly interpolated oscillator with sync status that allows changing the table number at k-rate.

## Description

oscilikts is the same as oscilikt. Except it has a sync input that can be used to re-initialize the oscillator to a k-rate phase value. It is slower than oscilikt and osciliktp.

## Syntax

    ares oscilikts xamp, xcps, kfn, async, kphs [, istor]

## Initialization

istor (optional, defaults to 0) -- skip initialization.

## Performance

xamp -- amplitude.

xcps -- frequency in Hz. Zero and negative values are allowed. However, the absolute value must be less than sr (and recommended to be less than sr/2).

kfn -- function table number. Can be varied at control rate (useful to “morph” waveforms, or select from a set of band-limited tables generated by GEN30).

async -- any positive value resets the phase of oscilikts to kphs. Zero or negative values have no effect.

kphs -- sets the phase, initially and when it is re-initialized with async.

## Examples

Here is an example of the oscilikts opcode. It uses the file oscilikts.csd.

Example 677. Example of the oscilikts opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o oscilikts.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; Initialize the global variables.
    sr = 44100
    kr = 4410
    ksmps = 10
    nchnls = 1

    ; Instrument #1: oscilikts example.
    instr 1
      ; Frequency envelope.
      kfrq expon 400, p3, 1200
      ; Phase.
      kphs line 0.1, p3, 0.9

      ; Sync 1
      atmp1 phasor 100
      ; Sync 2
      atmp2 phasor 150
      async diff 1 - (atmp1 + atmp2)

      a1 oscilikts 14000, kfrq, 1, async, 0
      a2 oscilikts 14000, kfrq, 1, async, -kphs

      out a1 - a2
    endin

    </CsInstruments>
    <CsScore>

    ; Table #1: Sawtooth wave
    f 1 0 3 -2 1 0 -1

    ; Play Instrument #1 for four seconds.
    i 1 0 4
    e

    </CsScore>
    </CsoundSynthesizer>

## See Also

oscilikt and osciliktp.

## Credits

Author: Istvan Varga

New in version 4.22

Prev | Up | Next
osciliktp | Home | osciln