lpsholdp
Prev | Orchestra Opcodes and Operators | Next

## lpsholdp

lpsholdp — Control signals based on held segments.

## Description

Generate control signal consisiting of held segments delimited by two or more specified points. The entire envelope can be looped at time-variant rate. Each segment coordinate can also be varied at k-rate.

## Syntax

    ksig lpsholdp  kphase, kvalue0, ktime0  [, kvalue1] [, ktime1] \
          [, kvalue2] [, ktime2] [...]

## Performance

ksig - output signal

kphase -- point of the sequence read, expressed as a fraction of a cycle (0 to 1)

kvalue0...kvalueN -- Values of points

ktime0...ktimeN -- Times between points; expressed in fractions of a cycle (see below). The final time designates a ramp between the final value and the first value.

lpsholdp opcode is similar to lpshold; the only difference is that, instead of frequency, a time-variant phase is required. If you use a phasor to get the phase value, you will have a behaviour identical to lpshold, but interesting results can be achieved when using phases having non-linear motions, making lpsholdp more powerful and general than lpshold.

## Examples

Here is an example of the lpsholdp opcode. It uses the file lpsholdp.csd.

Example 549. Example of the lpsholdp opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ; For Non-realtime ouput leave only the line below:
    ; -o lpsholdp.wav -W ;;; for file output any platform

    ; by Stefano Cucchi 2020

    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs = 1

    instr 1

    kphase1 phasor 3

    kmodulation oscil 0.5, 0.01, 2
    kphase2 phasor 3+kmodulation

    kamp linseg 0, 0.2, 1, p3-0.4, 1, 0.2, 0
    kfreq1  lpsholdp kphase1, cpspch(p4), 6, cpspch(p5), 10, cpspch(p6), 12
    kfreq2  lpsholdp kphase2, cpspch(p4), 6, cpspch(p5), 10, cpspch(p6), 12

    a1 = poscil(kamp, kfreq1, 1)
    a2 = poscil(kamp, kfreq2, 1)

    outch 1, a1
    outch 2, a2
    endin

    </CsInstruments>
    <CsScore>

    f1 0 8192 10 1 0 1 0 1 0 1 0 1 0 1
    f2 0 4096 10 1 0 1 1 1

    i1 0 10 6.09 6.02 7.03

    e

    </CsScore>
    </CsoundSynthesizer>

## Credits

Written by Gabriel Maldonado.

New in Csound 5 (Previously available only on CsoundAV)

Prev | Up | Next
lpshold | Home | lpslot