Experimental Orchestra Opcodes and GEN Routines
Prev | Part III. Reference | Next

## Experimental Orchestra Opcodes and GEN Routines

## Experimental Orchestra Opcodes

The following opcodes require a nVidia GPU to be present. They are distributed with the hope that they may be useful, and to encourage the use of parallelism in audio processing. Some of the new opcodes proform the same process as conventional existing does but some are new.

Prev | Up | Next
GENpadsynth | Home | cudanal