vphaseseg
Prev | Orchestra Opcodes and Operators | Next

## vphaseseg

vphaseseg — Allows one-dimensional HVS (Hyper-Vectorial Synthesis).

## Description

vphaseseg allows one-dimensional HVS (Hyper-Vectorial Synthesis).

## Syntax

    vphaseseg kphase, ioutab, ielems, itab1,idist1,itab2 \
          [,idist2,itab3, ... ,idistN-1,itabN]

## Initialization

ioutab - number of output table.

ielem - number of elements to process

itab1,...,itabN - breakpoint table numbers

idist1,...,idistN-1 - distances between breakpoints in percentage values

## Performance

kphase - phase pointer

vphaseseg returns the coordinates of section points of an N-dimensional space path. The coordinates of section points are stored into an output table. The number of dimensions of the N-dimensional space is determined by the ielem argument that is equal to N and can be set to any number. To define the path, user have to provide a set of points of the N-dimensional space, called break-points. Coordinates of each break-point must be contained by a different table. The number of coordinates to insert in each break-point table must obviously equal to ielem argument. There can be any number of break-point tables filled by the user.

Hyper-Vectorial Synthesis actually deals with two kinds of spaces. The first space is the N-dimensional space in which the path is defined, this space is called time-variant parameter space (or SPACE A). The path belonging to this space is covered by moving a point into the second space that normally has a number of dimensions smaller than the first. Actually, the point in motion is the projection of corresponding point of the N-dimensional space (could also be considered a section of the path). The second space is called user-pointer-motion space (or SPACE B) and, in the case of vphaseseg opcode, has only ONE DIMENSION. Space B is covered by means of kphase argument (that is a sort of path pointer), and its range is 0 to 1. The output corresponding to current pointer value is stored in ioutab table, whose data can be afterwards used to control any syntesis parameters.

In vphaseseg, each break-point is separated from the other by a distance expressed in percentage, where all the path length is equal to the sum of all distances. So distances between breakpoints can be different, differently from kinds of HVS in which space B has more than one dimension, in these cases distance between break-points MUST be THE SAME for all intervals.

## See Also

hvs1, hvs2, hvs3

## Credits

Author: Gabriel Maldonado

New in version 5.06

Prev | Up | Next
vosim | Home | vport