lpslot
Prev | Orchestra Opcodes and Operators | Next

## lpslot

lpslot — Selects the slot to be use by further lp opcodes.

## Description

Selects the slot to be use by further lp opcodes.

## Syntax

    lpslot islot

## Initialization

islot -- number of slot to be selected.

## Performance

lpslot selects the slot to be use by further lp opcodes. This is the way to load and reference several analyses at the same time.

## Examples

Here is a typical orc using the opcodes:

    ipower init 50000  ; Define sound generator
    ifreq  init 440
    asrc   buzz ipower, ifreq, 10, 1

    ktime  line 0, p3, p3              ; Define time lin
           lpslot 0                    ; Read square data poles
    krmsr, krmso, kerr, kcps lpread ktime,"square.pol"
           lpslot 1                    ; Read triangle data poles
    krmsr, krmso, kerr, kcps lpread ktime,"triangle.pol"
    kmix   line 0, p3, 1               ; Compute result of mixing
           lpinterp 0, 1, kmix         ; and balance power
    ares   lpreson asrc
    aout   balance ares, asrc
           out aout

## See Also

lpinterp

## Credits

Author: Mark Resibois
Brussels
1996

New in version 3.44

Prev | Up | Next
lpsholdp | Home | lufs