vps
Prev | Orchestra Opcodes and Operators | Next

## vps

vps — Shapes a phase signal according to a two-dimensional vector.

## Description

Vector phase shaping modifies a phase input value by mapping an input, in the range [0, 1) according to a non-linear function consisting of two piecewise linear segments joined at an inflection point. This is defined by the vector [kd, kv], where kd is in the range [0, 1) and kv can have any value.

## Syntax

    avp vps aph,kd,kv

## Performance

avp -- output phase.

aph -- input phase (as produced by phasor).

kd -- horizontal vector component.

aph -- vertical vector component.

## Examples

Here is an example of the use of the vps opcode. It uses the file vps.csd.

Example 1188. Example of the vps opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -o dac -d
    </CsOptions>
    <CsInstruments>
    0dbfs = 1
    nchnls=1
    ksmps = 1

    instr 1
     kd = oscili:k(0.5,2) + 0.5
     kv = oscili:k(0.5,1.5) + 0.5
     aph = vps(phasor(p5),kd,kv)
     asig = p4*tablei:a(aph,-1,1,0.25,1)
     out(linenr(asig,0.1,0.1,0.01))
    endin

    </CsInstruments>
    <CsScore>

    i 1 0 10 0.5 110

    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Victor Lazzarini
July 2020

Prev | Up | Next
vpowv_i | Home | vpvoc