trsplit
Prev | Orchestra Opcodes and Operators | Next

## trsplit

trsplit — Streaming partial track frequency splitting.

## Description

The trsplit opcode takes an input containg a TRACKS pv streaming signal (as generated, for instance by partials) and splits it into two signals according to a k-rate frequency 'split point'. The first output will contain all tracks up from 0Hz to the split frequency and the second will contain the tracks from the split frequency up to the Nyquist. It can also, optionally, scale the gain of the output signals by a k-rate amount (default 1). The result is two output signals containing only part of the original spectrum.

## Syntax

    fsiglow, fsighi trsplit fin, ksplit[, kgainlow, kgainhigh]

## Performance

fsiglow -- output pv stream in TRACKS format containing the tracks below the split point.

fsighi -- output pv stream in TRACKS format containing the tracks above and including the split point.

fin -- input pv stream in TRACKS format

ksplit -- frequency split point in Hz

kgainlow, kgainhig -- amplitude scaling of each one of the outputs (default 1).

## Examples

Here is an example of the trsplit opcode. It uses the file trsplit.csd.

Example 1117. Example of the trsplit opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o trsplit.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    ain	 diskin2 "beats.wav", 1
    fs1,fsi2 pvsifd  ain, 2048, 512, 1		; ifd analysis
    fst	 partials fs1, fsi2, .003, 1, 3, 500	; partial tracking
    fslo,fshi trsplit fst, 1500			; split partial tracks at 1500 Hz
    aout	 tradsyn fshi, 1, 1, 500, 1	; resynthesis of tracks above 1500Hz
             outs aout, aout

    endin
    </CsInstruments>
    <CsScore>
    f1 0 8192 10 1	;sine

    i 1 0 2
    e
    </CsScore>
    </CsoundSynthesizer>

The example above shows partial tracking of an ifd-analysis signal and linear additive resynthesis of the upper part of the spectrum (from 1500Hz).

## Credits

Author: Victor Lazzarini
February 2006

New in Csound 5.01

Prev | Up | Next
trshift | Home | turnoff