Operations Between a Vectorial and a Scalar Signal
Prev | Vectorial Opcodes | Next

## Operations Between a Vectorial and a Scalar Signal

These opcodes perform numeric operations between a vectorial control signal (hosted inside a function table), and a scalar signal. Result is a new vector that overrides old values of the table. There are k-rate and i-rate versions of the opcodes.

All these operators are designed to be used together with other opcodes that operate with vectorial signals such as vcella, adsynt, adsynt2, etc.

Operations Between a Vectorial and a Scalar Signal:

- vadd

- vmult

- vpow

- vexp

- vadd_i

- vmult_i

- vpow_i

- vexp_i

Prev | Up | Next
Vectorial Opcodes | Home | Operations Between two Vectorial Signals