lfsr
Prev | Orchestra Opcodes and Operators | Next

## lfsr

lfsr — Linear Feedback Shift Register (LFSR).

## Description

Output is a series of pseudo-random positive integers. This is the technique used in so-called "Turing machine" synth modules and is usually used to generate melodic sequences. This implementation is adapted from the firmware for the Ornament & Crime module, as used in the Quantermain and Meta-Q apps.

## Syntax

    knum lfsr ilen, iprob [, iseed]

## Initialization

ilen -- length of shift register, valid values are 1-31 (inclusive). The larger the length, the larger the resulting integers in the output. You can use this to constrain the output to a suitable range.

iprob -- probability, valid values 1-255 (inclusive). Controls the spread of the output; larger values result in a wider spread of values.

iseed (optional, default -1) -- initial state of the shift register, as a pattern of bits. The value is treated as an unsigned integer, so the default of -1 is effectivly all bits on (0b11111111...).

## Performance

knum -- integer output

## Examples

Here is an example of the lfsr opcode. It uses the file lfsr.csd.

Example 492. Example of the lfsr opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -W -o lfsr.wav
    </CsOptions>

    <CsInstruments>

    sr = 44100
    ksmps = 1
    nchnls = 2
    0dbfs = 1.0

    ; triangle wave
    gitabsz init 2^13
    giTri ftgen 1, 0, gitabsz, 7, 0, gitabsz/4, 1, gitabsz/2, -1, gitabsz/4, 0

    ; Grady Centaur scale
    giCent = ftgen(100, 0, 128, -51,
                   12, 2, 297.989, 60,
                   1.0, 21/20, 9/8, 7/6, 5/4, 4/3, 7/5, 3/2, 14/9, 5/3, 7/4, 15/8, 2.0)

    ; just print the values
    instr 1
        kn = lfsr(5, 128)
        printk2(kn)
    endin

    ; play a melodic sequence
    instr 2
        idur = p3
        iamp = p4
        iwav = p5
        itun = p6

        ; keep range small and transpose up 2 octaves to ensure audibility
        ; we're interpreting these number like MIDI notes numbers for easy table lookups
        kidx = lfsr(5, 128) + 24

        ktrig = metro(1)
        schedkwhen(ktrig, 0, 1, 3, 0, 1, iamp, iwav, itun, kidx)
    endin

    instr 3
        idur = p3
        iamp = ampdb(p4)
        iwav = p5
        itun = p6
        inote = p7

    	kenv = linen(iamp, 0.1, idur, 0.1)
    	aout = poscil3(kenv, tablekt(inote, itun), iwav)
    	outs(aout, aout)
    endin

    </CsInstruments>
    <CsScore>
    i 1 0 0.25
    i 2 0 10 -6 1 100

    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

By: Dave Seidel 2020

Based on code by Patrick Dowling in the Ornament & Crime firmware.

New in version 6.16

Prev | Up | Next
lfo | Home | limit