inletf
Prev | Orchestra Opcodes and Operators | Next

## inletf

inletf — Receives an frate signal (fsig) into an instrument from a named port.

## Description

Plugin opcode in signalflowgraph

Receives an frate signal (fsig) into an instrument from a named port.

## Syntax

    fsignal inletf Sname

## Initialization

Sname -- String name of the inlet port. The name of the inlet is implicitly qualified by the instrument name or number, so it is valid to use the same inlet name in more than one instrument (but not to use the same inlet name twice in one instrument).

## Performance

ksignal -- frate input signal

During performance, the frate inlet signal is received from each instance of an instrument containing an outlet port to which this inlet has been connected using the connect opcode. The signals of all the outlets connected to an inlet are combined in the inlet.

## See Also

outleta outletk outletkid outletf inleta inletk inletkid connect alwayson ftgenonce

## Credits

By: Michael Gogins 2009

Prev | Up | Next
inletkid | Home | inletv