octmidinn
Prev | Orchestra Opcodes and Operators | Next

## octmidinn

octmidinn — Converts a Midi note number value to octave-point-decimal.

## Description

Converts a Midi note number value to octave-point-decimal.

## Syntax

    octmidinn (MidiNoteNumber)  (init- or control-rate args only)

where the argument within the parentheses may be a further expression.

## Performance

octmidinn is a function that takes an i-rate or k-rate value representing a Midi note number and returns the equivalent pitch value in Csound's octave-point-decimal format. This conversion assumes that Middle C (8.000 in oct) is Midi note number 60. Midi note number values are typically integers in the range from 0 to 127 but fractional values or values outside of this range will be interpreted consistently.

| octmidinn vs. octmidi
The octmidinn opcode may be used in any Csound instrument instance whether it is activated from a Midi event, score event, line event, or from another instrument. The input value for octmidinn might for example come from a p-field in a textual score or it may have been retrieved from the real-time Midi event that activated the current note using the notnum opcode. You must specify an i-rate or k-rate expression for the Midi note number that is to be converted. On the other hand, the octmidi opcode only produces meaningful results in a Midi-activated note (either real-time or from a Midi score with the -F flag). With octmidi, the Midi note number value is taken from the Midi event associated with the instrument instance, and no location or expression for this value may be specified.

octmidinn and its related opcodes are really value converters with a special function of manipulating pitch data.

Data concerning pitch and frequency can exist in any of the following forms:

Table 17. Pitch and Frequency Values

Name | Abbreviation
--- | ---
octave point pitch-class (8ve.pc) | pch
octave point decimal | oct
cycles per second | cps
Midi note number (0-127) | midinn

The first two forms consist of a whole number, representing octave registration, followed by a specially interpreted fractional part. For pch, the fraction is read as two decimal digits representing the 12 equal-tempered pitch classes from .00 for C to .11 for B. For oct, the fraction is interpreted as a true decimal fractional part of an octave. The two fractional forms are thus related by the factor 100/12. In both forms, the fraction is preceded by a whole number octave index such that 8.00 represents Middle C, 9.00 the C above, etc. Midi note number values range between 0 and 127 (inclusively) with 60 representing Middle C, and are usually whole numbers. Thus A440 can be represented alternatively by 440 (cps), 69 (midinn), 8.09 (pch), or 8.75 (oct). Microtonal divisions of the pch semitone can be encoded by using more than two decimal places.

The mnemonics of the pitch conversion units are derived from morphemes of the forms involved, the second morpheme describing the source and the first morpheme the object (result). Thus cpspch(8.09) will convert the pitch argument 8.09 to its cps (or Hertz) equivalent, giving the value of 440. Since the argument is constant over the duration of the note, this conversion will take place at i-time, before any samples for the current note are produced.

By contrast, the conversion cpsoct(8.75 + k1) which gives the value of A440 transposed by the octave interval k1. The calculation will be repeated every k-period since that is the rate at which k1 varies.

| Note
The conversion from pch, oct, or midinn into cps is not a linear operation but involves an exponential process that could be time-consuming when executed repeatedly. Csound now uses a built-in table lookup to do this efficiently, even at audio rates. Because the table index is truncated without interpolation, pitch resolution when using one of these opcodes is limited to 8192 discrete and equal divisions of the octave, and some pitches of the standard 12-tone equally-tempered scale are very slightly mistuned (by at most 0.15 cents).

## Examples

Here is an example of the octmidinn opcode. It uses the file cpsmidinn.csd.

Example 664. Example of the octmidinn opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    ; Prints a table showing the equivalents of all Midi
    ; note numbers from 0-127 in cycles-per-second,
    ; octave.decimal, and octave.pitchclass units.

    <CsOptions>
    ; Select audio/midi flags here according to platform.
    ; This example produces no audio, so we render in
    ; non-realtime and turn off sound to disk:
    -n
    </CsOptions>
    <CsInstruments>

    instr 1
      ; i-time loop to print conversion table
      imidiNN =   0
      loop1:
        icps  = cpsmidinn(imidiNN)
        ioct  = octmidinn(imidiNN)
        ipch  = pchmidinn(imidiNN)

        print   imidiNN, icps, ioct, ipch

        imidiNN = imidiNN + 1
      if (imidiNN < 128) igoto loop1
    endin

    instr 2
      ; test k-rate converters
      kMiddleC  =   60
      kcps  = cpsmidinn(kMiddleC)
      koct  = octmidinn(kMiddleC)
      kpch  = pchmidinn(kMiddleC)

      printks "%d %f %f %f\n", 1.0, kMiddleC, kcps, koct, kpch
    endin

    </CsInstruments>
    <CsScore>
    i1 0 0
    i2 0 0.1
    e

    </CsScore>
    </CsoundSynthesizer>

## See Also

cpsmidinn, pchmidinn, octmidi, notnum, cpspch, cpsoct, octcps, octpch, pchoct

## Credits

Derived from original value converters by Barry Vercoe.

New in version 5.07

Prev | Up | Next
octmidib | Home | octpch