Operations Between two Vectorial Signals
Prev | Vectorial Opcodes | Next

## Operations Between two Vectorial Signals

These opcodes perform operations between two vectors, that is, each element of the first vector is processed with the corresponding element of the other vector. The result is a new vector that overrides the old values of the source vector.

Operations Between two Vectorial Signals:

- vaddv

- vsubv

- vmultv

- vdivv

- vpowv

- vexpv

- vcopy

- vmap

- vaddv_i

- vsubv_i

- vmultv_i

- vdivv_i

- vpowv_i

- vexpv_i

- vcopy_i

All these operators are designed to be used together with other opcodes that operate with vectorial signals such as vcella, adsynt, adsynt2, etc.

Prev | Up | Next
Operations Between a Vectorial and a Scalar Signal | Home | Vectorial Envelope Generators