gendyc
Prev | Orchestra Opcodes and Operators | Next

## gendyc

gendyc — Dynamic stochastic approach to waveform synthesis using cubic interpolation.

## Description

Implementation with cubic interpolation of the Génération Dynamique Stochastique (GENDYN), a dynamic stochastic approach to waveform synthesis conceived by Iannis Xenakis.

## Syntax

    ares gendyc kamp, kampdist, kdurdist, kadpar, kddpar, kminfreq, kmaxfreq, \
                kampscl, kdurscl [, initcps] [, knum]

    kres gendyc kamp, kampdist, kdurdist, kadpar, kddpar, kminfreq, kmaxfreq, \
                kampscl, kdurscl [, initcps] [, knum]

## Initialization

initcps (optional, default=12) -- max number of control points.

## Performance

kamp -- amplitude.

kampdist -- choice of probability distribution for the next perturbation of the amplitude of a control point. The valid distributions are:

- 0 - LINEAR

- 1 - CAUCHY

- 2 - LOGIST

- 3 - HYPERBCOS

- 4 - ARCSINE

- 5 - EXPON

- 6 - SINUS (external k-rate signal)

If kampdist=6, the user can use an external k-rate signal through kadpar.

kdurdist -- choice of distribution for the perturbation of the current inter control point duration. See kampdist for the valid distributions. If kdurdist=6, the user can use an external k-rate signal through kddpar.

kadpar -- parameter for the kampdist distribution. Should be in the range of 0.0001 to 1.

kddpar -- parameter for the kdurdist distribution. Should be in the range of 0.0001 to 1.

kminfreq -- minimum allowed frequency of oscillation.

kmaxfreq -- maximum allowed frequency of oscillation.

kampscl -- multiplier for the distribution's delta value for amplitude (1.0 is full range).

kdurscl -- multiplier for the distribution's delta value for duration.

knum (optional, default=initcps) -- current number of utilized control points.

The waveform is generated by knum - 1 segments and is repeated in the time. The vertexes (control points) are moved according to a stochastic action and they are limited within the boundaries of a mirror formed by an amplitude barrier and a time barrier.

## Examples

Here is an example of the gendyc opcode. It uses the file gendyc.csd.

Example 412. Example of the gendyc opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o oscil.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    aout gendyc 0.5, 1, 1, 1, 1, 220, 440, 0.5, 0.5
    outs aout, aout

    endin
    </CsInstruments>
    <CsScore>
    i1 0 10
    e
    </CsScore>
    </CsoundSynthesizer>

## References

1. Formalized Music (1992, Stuyvesant, NY: Pendragon Press), pp. 246 - 254, 289 - 322.

## See Also

gendy gendyx

## Credits

Based on Nick Collins's Gendy1 and Bhob Rainey's Gendy4 (SuperCollider)
Author: Tito Latini
January 2012

New in Csound version 5.16

Prev | Up | Next
gendy | Home | gendyx