outletf
Prev | Orchestra Opcodes and Operators | Next

## outletf

outletf — Sends a frate signal (fsig) out from an instrument to a named port.

## Description

Plugin opcode in signalflowgraph

Sends a frate signal (fsig) out from an instrument to a named port.

## Syntax

    outletf Sname, fsignal

## Initialization

Sname -- String name of the outlet port. The name of the outlet is implicitly qualified by the instrument name or number, so it is valid to use the same outlet name in more than one instrument (but not to use the same outlet name twice in one instrument).

## Performance

fsignal -- frate output signal (fsig)

During performance, the output signal is sent to each instance of an instrument containing an inlet port to which this outlet has been connected using the connect opcode. The signals of all the outlets connected to an inlet are combined in the inlet.

## See Also

outleta outletk outletkid inleta inletk inletkid inletf connect alwayson ftgenonce

## Credits

By: Michael Gogins 2009

Prev | Up | Next
outleta | Home | outletk