madsr
Prev | Orchestra Opcodes and Operators | Next

## madsr

madsr — Calculates the classical ADSR envelope using the linsegr mechanism.

## Description

Calculates the classical ADSR envelope using the linsegr mechanism.

## Syntax

    ares madsr iatt, idec, islev, irel [, idel] [, ireltim]

    kres madsr iatt, idec, islev, irel [, idel] [, ireltim]

## Initialization

iatt -- duration of attack phase

idec -- duration of decay

islev -- level for sustain phase

irel -- duration of release phase.

idel -- period of zero before the envelope starts

ireltim (optional, default=-1) -- Control release time after receiving a MIDI noteoff event. If less than zero, the longest release time given in the current instrument is used. If zero or more, the given value will be used for release time. Its default value is -1. (New in Csound 3.59 - not yet properly tested)

Please note that the release time was restricted to 32767/kr seconds in versions prior to 5.00; since then it has been (231-1)/kr.

## Performance

The envelope is in the range 0 to 1 and may need to be scaled further. The envelope may be described as:

Picture of an ADSR envelope.

The length of the sustain is calculated from the length of the note. This means adsr is not suitable for use with MIDI events. The opcode madsr uses the linsegr mechanism, and so can be used in MIDI applications.

You can use other pre-made envelopes which start a release segment upon receiving a note off message, like linsegr and expsegr, or you can construct more complex envelopes using xtratim and release. Note that you do not need to use xtratim if you are using madsr, since the time is extended automatically.

| Note
Times for iatt, idec and irel cannot be 0. If 0 is used, no envelope is generated. Use a very small value like 0.0001 if you need an instantaneous attack, decay or release.

## Examples

Here is an example of the madsr opcode. It uses the file madsr.csd.

Example 553. Example of the madsr opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o madsr.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    /* Written by Iain McCurdy */
    ; Initialize the global variables.
    sr = 44100
    kr = 441
    ksmps = 100
    nchnls = 1

    ; Instrument #1.
    instr 1
      ; Attack time.
      iattack = 0.5
      ; Decay time.
      idecay = 0
      ; Sustain level.
      isustain = 1
      ; Release time.
      irelease = 0.5
      aenv madsr iattack, idecay, isustain, irelease

      a1 oscili 10000, 440, 1
      out a1*aenv
    endin

    </CsInstruments>
    <CsScore>

    /* Written by Iain McCurdy */
    ; Table #1, a sine wave.
    f 1 0 1024 10 1

    ; Leave the score running for 6 seconds.
    f 0 6

    ; Play Instrument #1 for two seconds.
    i 1 0 2
    e

    </CsScore>
    </CsoundSynthesizer>

Here is another example of the madsr opcode, using midi input. It uses the file madsr-2.csd.

Example 554. second example of the madsr opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  -m0  --midi-key=4 --midi-velocity-amp=5 ; treat p4 and p5 as midi data
    ; For Non-realtime ouput leave only the line below:
    ; -o madsr-2.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    ; by Menno Knevel - 2021

    instr 1	                              ; use score and treat p4 and p5 as midi data
    icps    = cpsmidinn(p4)               ; take midi note (p4) from score
    iveloc  ampmidid p5, 92               ; take velocity (p5) from score
    ;               att, dec, lvl, release
    kenv    madsr  .001, .2,   1,    p6
    prints  "duration of note (%ds) + release (%2.1fs)\\n", p3, p6                ;
    asig    vco2    iveloc, icps
    asig    butlp   asig, 2000
            outs    asig*kenv, asig*kenv
    endin

    </CsInstruments>
    <CsScore>
    ;      note vel release
    s
    i 1 0 1 62  60  0
    i 1 2 1 62  80  0
    i 1 4 1 62  100 0
    i 1 6 1 58  50  0
    s
    i 1 1 1 62  60  0
    i 1 3 1 62  80  .5
    i 1 5 1 62  100 1.5
    i 1 7 1 58  50  3
    e
    </CsScore>
    </CsoundSynthesizer>

Here is an example for the adsr-group, comparing the different adsr opcodes. It uses the file adsr-group.csd.

Example 555. Example of the adsr group.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac    ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o adsr-group.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; by Menno Knevel - 2021

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    ; both amplitude and filter use same ADSR curves
    instr 1
    kenv	adsr	.01, .5, .5, p4    	; linear envelope
    asig	vco2	kenv, 110			; A+D+S+R = p3
    asig	rezzy	asig, 500+(kenv*1000), 10	; same curve but scaled
    		outs	asig, asig
    endin

    instr 2	; midi behavior
    kenv	madsr	.01, .5, .5, p4		; linear envelope
    asig	vco2	kenv, 110			; A+D+S = p3, then go into Release stage
    asig	rezzy	asig, 500+(kenv*1000), 10	; same curve but scaled
    		outs	asig, asig
    endin

    instr 3
    kenv	xadsr	.01, .5 , .5, p4    ; exponential envelope
    asig	vco2	kenv, 110			; A+D+S+R = p3
    asig	rezzy	asig, 500+(kenv*1000), 10	; same curve but scaled
    		outs	asig, asig
    endin

    instr 4	; midi behavior
    kenv	mxadsr	.01, .5 , .5, p4	; exponential envelope
    asig	vco2	kenv, 110			; A+D+S = p3, then go into Release stage
    asig	rezzy	asig, 500+(kenv*1000), 10	; same curve but scaled
    		outs	asig, asig
    endin

    </CsInstruments>
    <CsScore>
    s
    i1 1 2 .01	; same notes for everyone!
    i1 5 . .5
    i1 9 . 1.5
    s
    i2 1 2 .01
    i2 5 . .5
    i2 9 . 1.5
    s
    i3 1 2 .01
    i3 5 . .5
    i3 9 . 1.5
    s
    i4 1 2 .01
    i4 5 . .5
    i4 9 . 1.5
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

linsegr, expsegr, envlpxr, mxadsr, madsr, xadsr expon, expseg, expsega line, linseg, xtratim

## Credits

Author: John ffitch

November 2002. Thanks to Rasmus Ekman, added documentation for the ireltim parameter.

December 2002. Thanks to Iain McCurdy, added an example.

December 2002. Thanks to Istvan Varga, added documentation about the maximum release time.

New in Csound version 3.49.

Prev | Up | Next
maca | Home | mags