butterhp
Prev | Orchestra Opcodes and Operators | Next

## butterhp

butterhp — A high-pass Butterworth filter.

## Description

Implementation of second-order high-pass Butterworth filter. This opcode can also be written as buthp.

## Syntax

    ares butterhp asig, kfreq [, iskip]

    ares butterhp asig, afreq [, iskip]

## Initialization

iskip (optional, default=0) -- Skip initialization if present and non-zero.

## Performance

These filters are Butterworth second-order IIR filters. They are slightly slower than the original filters in Csound, but they offer an almost flat passband and very good precision and stopband attenuation.

asig -- Input signal to be filtered.

kfreq/afreq -- Cutoff or center frequency for each of the filters.

## Examples

Here is an example of the butterhp opcode. It uses the file butterhp.csd.

Example 108. Example of the butterhp opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;RT audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o butterhp.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs = 1

    instr 1	  ; White noise

    asig rand 0.5
    outs asig, asig

    endin

    instr 2	; filtered noise

    asig rand 0.6
    ahp  butterhp asig, 500  ;pass frequencies above 500 Hz
         outs ahp, ahp

    endin

    </CsInstruments>
    <CsScore>

    i 1 0 2
    i 2 2.5 2
    e

    </CsScore>
    </CsoundSynthesizer>

## See Also

butterbp, butterbr, butterlp

## Credits

Author: Paris Smaragdis
MIT, Cambridge
1995

Existed in 3.30

Audio rate parameters introduced in version 6.02

October 2013.

Prev | Up | Next
butterbr | Home | butterlp