tabrec
Prev | Orchestra Opcodes and Operators | Next

## tabrec

tabrec — Recording of control signals.

## Description

Records control-rate signals on trigger-temporization basis.

## Syntax

    tabrec   ktrig_start, ktrig_stop, knumtics, kfn, kin1 [,kin2,...,kinN]

## Performance

ktrig_start -- start recording when non-zero.

ktrig_stop -- stop recording when knumtics trigger impulses are received by this input argument.

knumtics -- stop recording or reset playing pointer to zero when the number of tics defined by this argument is reached.

kfn -- table where k-rate signals are recorded.

kin1,...,kinN -- input signals to record.

The tabrec and tabplay opcodes allow to record/playback control signals on trigger-temporization basis.

tabrec opcode records a group of k-rate signals by storing them into kfn table. Each time ktrig_start is triggered, tabrec resets the table pointer to zero and begins to record. Recording phase stops after knumtics trigger impulses have been received by ktrig_stop argument.

These opcodes can be used like a sort of ``middle-term'' memory that ``remembers'' generated signals. Such memory can be used to supply generative music with a coherent iterative compositional structure.

## Examples

Here is an example of the tabrec opcode. It uses the file tabrec.csd.

Example 1072. Example of the tabrec opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o oscil.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    gifn ftgen 0,0,1049576,2,0

    ; record control signals
    instr 1
    ktrig_start init    1
    koct        rspline 7,10,1,2
    kpan        rspline 7,10,0.1,0.9
    ktrig_stop  =       1
    knumtics    =       kr*p3
                tabrec  ktrig_start,ktrig_stop,knumtics,gifn,koct,kpan
    ktrig_start =   0
    endin

    ; play control signals
    instr 2
    koct,kpan   init    0
    ktrig       init    1
    knumtics    =       kr*p3
                tabplay ktrig,knumtics,gifn,koct,kpan

    ktrig       =       0

    asig        poscil 0.1, cpsoct(koct)
    aL,aR       pan2    asig,kpan
                outs    aL,aR
    endin

    </CsInstruments>

    <CsScore>
    i1 0 10
    i2 2 10
    i2 4 10
    e

    </CsScore>

    </CsoundSynthesizer>

## See Also

tabplay

## Credits

Written by Gabriel Maldonado.

Example written by Iain McCurdy

Prev | Up | Next
tabplay | Home | tabsum