delayr
Prev | Orchestra Opcodes and Operators | Next

## delayr

delayr — Reads from an automatically established digital delay line.

## Description

Reads from an automatically established digital delay line.

## Syntax

    ares delayr idlt [, iskip]

## Initialization

idlt -- requested delay time in seconds. This can be as large as available memory will permit. The space required for n seconds of delay is 4n * sr bytes. It is allocated at the time the instrument is first initialized, and returned to the pool at the end of a score section.

iskip (optional, default=0) -- initial disposition of delay-loop data space (see reson). The default value is 0.

## Performance

delayr reads from an automatically established digital delay line, in which the signal retrieved has been resident for idlt seconds. This unit must be paired with and precede an accompanying delayw unit. Any other Csound statements can intervene.

## Examples

Here is an example of the delayr opcode. It uses the file delayr.csd.

Example 214. Example of the delayr opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;RT audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o delayr.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs = 1

    gasig  init 0
    gidel  = 1		;delay time in seconds

    instr 1

    ain  pluck .7, 440, 1000, 0, 1
         outs ain, ain

    vincr gasig, ain	;send to global delay
    endin

    instr 2

    ifeedback = p4

    abuf2	delayr	gidel
    adelL 	deltap	.4		;first tap (on left channel)
    adelM 	deltap	1		;second tap (on middle channel)
    	delayw	gasig + (adelL * ifeedback)

    abuf3	delayr	gidel
    kdel	line    1, p3, .01	;vary delay time
    adelR 	deltap  .65 * kdel	;one pitch changing tap (on the right chn.)
    	delayw	gasig + (adelR * ifeedback)
    ;make a mix of all deayed signals
    	outs	adelL + adelM, adelR + adelM

    clear	gasig
    endin

    </CsInstruments>
    <CsScore>

    i 1 0 1
    i 1 3 1
    i 2 0 3  0	;no feedback
    i 2 3 8 .8	;lots of feedback
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

delay, delay1, delayw

Prev | Up | Next
delayk | Home | delayw