sliderKawai
Prev | Orchestra Opcodes and Operators | Next

## sliderKawai

sliderKawai — Creates a bank of 16 different MIDI control message numbers from a KAWAI MM-16 midi mixer.

## Description

Creates a bank of 16 different MIDI control message numbers from a KAWAI MM-16 midi mixer.

## Syntax

    k1, k2, ...., k16 sliderKawai imin1, imax1, init1, ifn1, \
          imin2, imax2, init2, ifn2, ..., imin16, imax16, init16, ifn16

## Initialization

imin1 ... imin16 -- minimum values for each controller

imax1 ... imax16 -- maximum values for each controller

init1 ... init16 -- initial value for each controller

ifn1 ... ifn16 -- function table for conversion for each controller

## Performance

k1 ... k16 -- output values

The opcode sliderKawai is equivalent to slider16, but it has the controller and channel numbers (ichan and ictlnum) hard-coded to make for quick compatiblity with the KAWAI MM-16 midi mixer. This device doesn't allow changing the midi message associated to each slider. It can only output on control 7 for each fader on a separate midi channel. This opcode is a quick way of assigning the mixer's 16 faders to k-rate variables in csound.

## See Also

slider16, slider16f, slider32, slider32f, slider64, slider64f, slider8, slider8f

## Credits

Author: Gabriel Maldonado

New in Csound version 5.06

Prev | Up | Next
slider8tablef | Home | sndloop