chn
Prev | Orchestra Opcodes and Operators | Next

## chn

chn — Declare a channel of the named software bus.

## Description

Declare a channel of the named software bus, with setting optional parameters in the case of a control channel. If the channel does not exist yet, it is created, with an inital value of zero or empty string. Otherwise, the type (control, audio, or string) of the existing channel must match the declaration, or an init error occurs. The input/output mode of an existing channel is updated so that it becomes the bitwise OR of the previous and the newly specified value.

## Syntax

     chn_k Sname, imode[, itype, idflt, imin, ima, ix, iy,
          iwidth, iheight, Sattributes]

     chn_a Sname, imode

     chn_S Sname, imode

     chn_S Sname, Smode

## Initialization

imode -- sum of at least one of 1 for input and 2 for output.

Smode -- The mode can also be set with a string: "r" for input, "w" for output or "rw" for input/output

itype (optional, defaults to 0) -- channel subtype for control channels only. Possible values are:

- 0: default/unspecified (idflt, imin, and imax are ignored)

- 1: integer values only

- 2: linear scale

- 3: exponential scale

idflt (optional, defaults to 0) -- default value, for control channels with non-zero itype only. Must be greater than or equal to imin, and less than or equal to imax.

imin (optional, defaults to 0) -- minimum value, for control channels with non-zero itype only. Must be non-zero for exponential scale (itype = 3).

imax (optional, defaults to 0) -- maximum value, for control channels with non-zero itype only. Must be greater than imin. In the case of exponential scale, it should also match the sign of imin.

ix -- suggested x position for controller.

iy -- suggested y position for controller.

iwidth -- suggested width position for controller.

iheight -- suggested height position for controller.

Sattributes -- attributes for controller.

## Notes

The channel parameters (imode, itype, idflt, imin, and imax) are only hints for the host application or external software accessing the bus through the API, and do not actually restrict reading from or writing to the channel in any way. Also, the initial value of a newly created control channel is zero, regardless of the setting of idflt.

For communication with external software, using chnexport may be preferred, as it allows direct access to orchestra variables exported as channels of the bus, eliminating the need for using chnset and chnget to send or receive data.

## Performance

chn_k, chn_a, and chn_S declare a control, audio, or string channel, respectively.

## Example

The example shows the software bus being used as an asynchronous control signal to select a filter cutoff. It assumes that an external program that has access to the API is feeding the values.

            sr = 44100
            kr = 100
            ksmps = 1

            chn_k "cutoff", 1, 3, 1000, 500, 2000

            instr   1
               kc   chnget    "cutoff"
               a1   oscil     p4, p5, 100
               a2   lowpass2  a1, kc, 200
                    out       a2
            endin

## Credits

Author: Istvan Varga
2005

Prev | Up | Next
checkbox | Home | chnclear