tbvcf
Prev | Orchestra Opcodes and Operators | Next

## tbvcf

tbvcf — Models some of the filter characteristics of a Roland TB303 voltage-controlled filter.

## Description

This opcode attempts to model some of the filter characteristics of a Roland TB303 voltage-controlled filter. Euler's method is used to approximate the system, rather than traditional filter methods. Cutoff frequency, Q, and distortion are all coupled. Empirical methods were used to try to unentwine, but frequency is only approximate as a result. Future fixes for some problems with this opcode may break existing orchestras relying on this version of tbvcf.

## Syntax

    ares tbvcf asig, xfco, xres, kdist, kasym [, iskip]

## Initialization

iskip (optional, default=0) -- if non zero skip the initialisation of the filter. (New in Csound version 4.23f13 and 5.0)

## Performance

asig -- input signal. Should be normalized to ±1.

xfco -- filter cutoff frequency. Optimum range is 10,000 to 1500. Values below 1000 may cause problems.

xres -- resonance or Q. Typically in the range 0 to 2.

kdist -- amount of distortion. Typical value is 2. Changing kdist significantly from 2 may cause odd interaction with xfco and xres.

kasym -- asymmetry of resonance. Typically in the range 0 to 1.

## Examples

Here is an example of the tbvcf opcode. It uses the file tbvcf.csd.

Example 1082. Example of the tbvcf opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in    No messages
    -odac           -iadc     -d     ;;;RT audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; -o tbvcf.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ;---------------------------------------------------------
    ; TBVCF Test
    ; Coded by Hans Mikelson December, 2000
    ;---------------------------------------------------------
      sr =  44100   ; Sample rate
      ksmps =  10   ; Samples/Kontrol period
      nchnls =  2        ; Normal stereo
      0dbfs = 1

              instr 10

      idur	=	p3			; Duration
      iamp	=	p4			; Amplitude
      ifqc	=	cpspch(p5)		; Pitch to frequency
      ipanl	=	sqrt(p6)		; Pan left
      ipanr	=	sqrt(1-p6)		; Pan right
      iq	=	p7
      idist	=	p8
      iasym =	p9

    kdclck		linseg	0, .002, 0.9, idur-.004, 0.9, .002, 0	; Declick envelope
    kfco		expseg	10000, idur, 1000			; Frequency envelope
    ax		vco		1, ifqc, 2, 0.5			; Square wave
    ay		tbvcf		ax, kfco, iq, idist, iasym		; TB-VCF
    ay		buthp	ay/1, 100				; Hi-pass

    		outs		ay*iamp*ipanl*kdclck, ay*iamp*ipanr*kdclck
              endin

    </CsInstruments>
    <CsScore>

    f1 0 65536 10 1

    ; TeeBee Test
    ;   Sta  Dur  Amp    Pitch Pan  Q    Dist1 Asym
    i10 0    0.2  0.5    7.00  .5   0.0  2.0   0.0
    i10 0.3  0.2  0.5    7.00  .5   0.8  2.0   0.0
    i10 0.6  0.2  0.5    7.00  .5   1.6  2.0   0.0
    i10 0.9  0.2  0.5    7.00  .5   1.7  2.0   0.0
    i10 1.2  0.2  0.5    7.00  .5   1.8  2.0   0.0
    i10 1.8  0.2  0.5    7.00  .5   0.0  2.0   0.25
    i10 2.1  0.2  0.5    7.00  .5   0.8  2.0   0.25
    i10 2.4  0.2  0.5    7.00  .5   1.6  2.0   0.25
    i10 2.7  0.2  0.5    7.00  .5   1.8  2.0   0.25
    i10 3.0  0.2  0.5    7.00  .5   1.9  2.0   0.25
    i10 3.3  0.2  0.5    7.00  .5   2.0  2.0   0.25
    i10 3.6  0.2  0.5    7.00  .5   0.0  2.0   0.5
    i10 3.9  0.2  0.5    7.00  .5   0.8  2.0   0.5
    i10 4.2  0.2  0.5    7.00  .5   1.6  2.0   0.5
    i10 4.5  0.2  0.5    7.00  .5   1.8  2.0   0.5
    i10 4.8  0.2  0.5    7.00  .5   1.9  2.0   0.5
    i10 5.1  0.2  0.5    7.00  .5   2.0  2.0   0.5
    i10 5.4  0.2  0.5    7.00  .5   0.0  2.0   0.75
    i10 5.7  0.2  0.5    7.00  .5   0.8  2.0   0.75
    i10 6.0  0.2  0.5    7.00  .5   1.6  2.0   0.75
    i10 6.3  0.2  0.5    7.00  .5   1.8  2.0   0.75
    i10 6.6  0.2  0.5    7.00  .5   1.9  2.0   0.75
    i10 6.9  0.2  0.5    7.00  .5   2.0  2.0   0.75
    i10 7.2  0.2  0.5    7.00  .5   0.0  2.0   1.0
    i10 7.5  0.2  0.5    7.00  .5   0.8  2.0   1.0
    i10 7.8  0.2  0.5    7.00  .5   1.6  2.0   1.0
    i10 8.1  0.2  0.5    7.00  .5   1.8  2.0   1.0
    i10 8.4  0.2  0.5    7.00  .5   1.9  2.0   1.0
    i10 8.7  0.2  0.5    7.00  .5   2.0  2.0   1.0
    e

    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Hans Mikelson
December, 2000 -- January, 2001

New in Csound 4.10

Prev | Up | Next
taninv2 | Home | tempest