sc_trig
Prev | Orchestra Opcodes and Operators | Next

## sc_trig

sc_trig — Timed trigger (Replaced by trighold)

## Description

Plugin opcode in scugens.

Timed trigger. Port of Supercollider's Trig ugen. This opcode is deprecated and renamed to trighold,

## Syntax

    aout sc_trig ain, kdur

    kout sc_trig kin, kdur

## Initialization

initialvalue If given, sets the internal state. Default=0

## Performance

ain -- Trigger. Trigger can be any signal. A trigger happens when the signal changes from non-positive to positive.

kdur -- Duration of the trigger in seconds.

When a nonpositive to positive transition occurs at the input, Trig outputs the level of the triggering input for the specified duration, otherwise it outputs zero.

## Examples

Here is an example of the sc_trig opcode. It uses the file sc_trig.csd.

Example 934. Example of the sc_trig opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 128
    nchnls = 2
    0dbfs = 1.0

    instr 1
      km = metro(1)
      kt timeinsts
      ktrig = sc_trig(km, 0.5)
      printks "t=%f  km=%f    ktrig=%f\n", 0.01, kt, km, ktrig
    endin

    instr 2
      am = upsamp(metro(1))
      aenv = sc_trig(am, 0.5)
      asig pinker
      outch 1, asig*aenv
      outch 2, asig
    endin

    </CsInstruments>
    <CsScore>
    i 1 0 10
    i 2 0 10

    </CsScore>
    </CsoundSynthesizer>

## See Also

sc_lag, metro, mpulse trigger

## Credits

By: Eduardo Moguillansky 2017

Prev | Up | Next
trigphasor | Home | trighold