vbapz
Prev | Orchestra Opcodes and Operators | Next

## vbapz

vbapz — Writes a multi-channel audio signal to a ZAK array.

## Description

Writes a multi-channel audio signal to a ZAK array.

## Syntax

    vbapz inumchnls, istartndx, asig, kazim [, kelev] [, kspread]

## Initialization

inumchnls -- number of channels to write to the ZA array. Must be in the range 2 - 256.

istartndx -- first index or position in the ZA array to use

## Performance

asig -- audio signal to be panned

kazim -- azimuth angle of the virtual source

kelev (optional) -- elevation angle of the virtual source

kspread (optional) -- spreading of the virtual source (range 0 - 100). If value is zero, conventional amplitude panning is used. When kspread is increased, the number of loudspeakers used in panning increases. If value is 100, the sound is applied to all loudspeakers.

The opcode vbapz is the multiple channel analog of the opcodes like vbap4, working on inumchnls and using a ZAK array for output.

| Warning
Please note that all vbap panning opcodes require the vbap system to be initialized using vbaplsinit.

## Examples

See the entry for vbap8 for an example of usage of the vbap opcodes.

## Reference

Ville Pulkki: “Virtual Sound Source Positioning Using Vector Base Amplitude Panning” Journal of the Audio Engineering Society, 1997 June, Vol. 45/6, p. 456.

## See Also

vbap16, vbap16move, vbap4, vbap4move, vbap8, vbap8move, vbaplsinit, vbapzmove

## Credits

John ffitch
University of Bath/Codemist Ltd.
Bath, UK
May 2000

New in Csound Version 4.07. Input parameters accept k-rate since Csund 5.09.

Prev | Up | Next
vbaplsinit | Home | vbapzmove