rect2pol
Prev | Orchestra Opcodes and Operators | Next

## rect2pol

rect2pol — Rectangular to polar format conversion.

## Description

Converts an input array in real-imaginary format to magnitude-phase format.

## Syntax

    kout[] rect2pol kin[]

## Performance

kout[] -- output array containing the complex-valued magnitude-phase output. It will be created if it does not exist.

kin[] -- input array containing the complex-valued real-imaginary input.

## Examples

Here is an example of the rect2pol opcode. It uses the file rect2pol.csd.

Example 877. Example of the rect2pol opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -d -o dac
    </CsOptions>
    <CsInstruments>
    /* ksmps needs to be an integer div of
       hopsize */
    ksmps = 64

    instr 1

     ihopsize = 256   ; hopsize
     ifftsize = 1024  ; FFT size
     iolaps = ifftsize/ihopsize ; overlaps
     ibw = sr/ifftsize ; bin bandwidth
     kcnt init 0    ; counting vars
     krow init 0

     kOla[] init ifftsize ; overlap-add buffer
     kIn[] init ifftsize  ; input buffer
     kOut[][] init iolaps, ifftsize ; output buffers

     a1 diskin2 "fox.wav",1,0,1 ; audio input

     /* every hopsize samples */
     if kcnt == ihopsize then
       /* window and take FFT */
       kWin[] window kIn,krow*ihopsize
       kSpec[] rfft kWin

       kSpec rect2pol kSpec

       /* reduce mags between high and low freqs */
       ilow = 0
       ihigh = 1000
       ki = int(ilow/ibw)
       until ki >= int(ihigh/ibw) do
         kSpec[ki] = kSpec[ki]*0.1
         ki += 2
       od

       kSpec pol2rect kSpec

       /* IFFT + window */
       kRow[] rifft kSpec
       kWin window kRow, krow*ihopsize
       /* place it on out buffer */
       kOut setrow kWin, krow

       /* zero the ola buffer */
       kOla = 0
       /* overlap-add */
       ki = 0
       until ki == iolaps do
         kRow getrow kOut, ki
         kOla = kOla + kRow
         ki += 1
       od

      /* update counters */
      krow = (krow+1)%iolaps
      kcnt = 0
     endif

     /* shift audio in/out of buffers */
     kIn shiftin a1
     a2 shiftout kOla
        out a2/iolaps

     /* increment counter */
     kcnt += ksmps

    endin

    </CsInstruments>
    <CsScore>
    i1 0 10
    </CsScore>
    </CsoundSynthesizer>

## See Also

Vectorial opcodes, array opcodes

## Credits

Author: Victor Lazzarini
NUI Maynooth
2014

New in version 6.04

Prev | Up | Next
readscratch | Home | reinit