GEN44
Prev | Score Statements and GEN Routines | Next

## GEN44

GEN44 — Generates a stiffness (connection) matrix for use in scanu/scanu2.

## Description

Generates a stiffness matrix from a text file of triples numbers.

## Syntax

    f # time size -44  "filename"

    f # time size -44  num

## Performance

The file named in version 1 or the file stiff.num in the second case is read to create the matrix.

The first line of the file should be “ <MATRIX size=integer> ” and it creates a square matrix of the indicated size. This is followed by lines of two or three numbers, the first two denoting a connection from the first to the second and the third is a weight. If the third is omitted it is taken as value 1. The list is terminated by a “ </MATRIX> ” line or end of file.

can be given as zero in which case a size*size table is created. If the size in the gen statememt is too small for the matrix then space is re-allocated to the required size.

## Examples

Here is an example of the GEN44 generator. It uses the file gen44.csd.

Example 1302. Example of the GEN44 generator.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 1
    0dbfs = 1

    instr scan

    a0 init 0

    irate = .01

    kmass line 2,p3,5
    kstiff line 30,p3,45
    kcenter line .08,p3,.01
    kdamp line .01,p3,.08
    kpos line 0,p3,16
    kdisplace line 0,p3,.5

    ;scanu2 init,irate,ifndisplace,ifnmass,ifnmatrix,ifncentr,ifndamp,kmass,kmtrxstiff,
    ; kcentr, kdamp, ileft, iright, kpos, kdisplace, ain, idisp, id
    scanu2 -1, irate, 6, 2, 3, 4, 5, kmass, kstiff, kcenter, kdamp, .2, .7, kpos,
    kdisplace, a0, 1, 2

    ;ar scans kamp, kfreq, ifntraj, id
    a1 scans ampdbfs(p4), cpspch(p5), 7, 2
    a1 dcblock2 a1
    out a1
    endin

    </CsInstruments>
    <CsScore>
    ; Initial displacement condition
    f1 0 16 10 1 ; sine hammer

    ; Masses
    f2 0 16 -7 1 16 1

    ; Spring matrices
    f3 0 0 -44 "string_with_extras-16.matrxT"

    ; Centering force
    f4 0 16 -7 1 16 1 ; uniform initial centering

    ; Damping
    f5 0 16 -7 1 16 1 ; uniform damping

    ; Initial displacement - (displacement, vel, and acceleration
    ; Acceleration is from stiffness matrix pos effect - increases acceleration
    f6 0 16 -7 .01 16 .01 ; uniform initial velocity-displacement

    ; Trajectories
    f7 0 16 -5 .001 16 16

    i"scan" 0 2 -6 7.00
    i"scan" 2 2 -6 5.00
    i"scan" 4 2 -6 6.00
    i"scan" 6 2 -6 8.00
    i"scan" 8 2 -6 10.00

    e

    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: John ffitch

New in Version 6.16 June 2021

Prev | Up | Next
GEN43 | Home | GEN49