inleta
Prev | Orchestra Opcodes and Operators | Next

## inleta

inleta — Receives an arate signal into an instrument through a named port.

## Description

Plugin opcode in signalflowgraph

Receives an arate signal into an instrument through a named port.

## Syntax

    asignal inleta Sname

## Initialization

Sname -- String name of the inlet port. The name of the inlet is implicitly qualified by the instrument name or number, so it is valid to use the same inlet name in more than one instrument (but not to use the same inlet name twice in one instrument).

## Performance

asignal -- audio input signal

During performance, the arate inlet signal is received from each instance of an instrument containing an outlet port to which this inlet has been connected using the connect opcode. The signals of all the outlets connected to an inlet are summed in the inlet.

## Examples

Here is an example of the inleta opcode. It uses the file inleta.csd.

Example 463. Example of the inleta opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o inleta.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2

    ; Connect up instruments and effects to create the signal flow graph.

    connect "SimpleSine",   "leftout", "Reverberator", "leftin"
    connect "SimpleSine",   "rightout","Reverberator", "rightin"

    connect "Moogy",        "leftout", "Reverberator", "leftin"
    connect "Moogy",        "rightout","Reverberator", "rightin"

    connect "Reverberator", "leftout", "Compressor",   "leftin"
    connect "Reverberator", "rightout","Compressor",   "rightin"

    connect "Compressor",   "leftout", "Soundfile",    "leftin"
    connect "Compressor",   "rightout","Soundfile",    "rightin"

    ; Turn on the "effect" units in the signal flow graph.

    alwayson "Reverberator", 0.91, 12000
    alwayson "Compressor"
    alwayson "Soundfile"

    ; Define instruments and effects in order of signal flow.

    instr SimpleSine
    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    ; Default values:   p1  p2  p3  p4  p5  p6  p7  p8  p9  p10
                    pset	        0,  0,  10, 0,  0,  0,  0.5
    iattack		= 0.015
    idecay		= 0.07
    isustain	= p3
    irelease	= 0.3
    p3		= iattack + idecay + isustain + irelease
    adamping	linsegr 0.0, iattack, 1.0, idecay + isustain, 1.0, irelease, 0.0
    iHz 		= cpsmidinn(p4)
    ; Rescale MIDI velocity range to a musically usable range of dB.
    iamplitude 	= ampdb(p5 / 127 * 15.0 + 60.0)
    ; Use ftgenonce instead of ftgen, ftgentmp, or f statement.
    icosine		ftgenonce 0, 0, 65537, 11, 1
    aoscili		oscili iamplitude, iHz, icosine
    aadsr 		madsr iattack, idecay, 0.6, irelease
    asignal 	= aoscili * aadsr
    aleft, aright	pan2 asignal, p7
    ; Stereo audio output to be routed in the orchestra header.
    		outleta "leftout", aleft
    		outleta "rightout", aright
    endin

    instr Moogy
    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    ; Default values:   p1  p2  p3  p4  p5  p6  p7  p8  p9  p10
    		pset            0,  0,  10, 0,  0,  0,  0.5
    iattack		= 0.003
    isustain	= p3
    irelease	= 0.05
    p3		= iattack + isustain + irelease
    adamping	linsegr	0.0, iattack, 1.0, isustain, 1.0, irelease, 0.0
    iHz 		= cpsmidinn(p4)
    ; Rescale MIDI velocity range to a musically usable range of dB.
    iamplitude 	= ampdb(p5 / 127 * 20.0 + 60.0)
    		print iHz, iamplitude
    ; Use ftgenonce instead of ftgen, ftgentmp, or f statement.
    isine 		ftgenonce 0, 0, 65537, 10, 1
    asignal 	vco iamplitude, iHz, 1, 0.5, isine
    kfco 		line 2000, p3, 200
    krez 		= 0.8
    asignal 	moogvcf asignal, kfco, krez, 100000
    asignal		= asignal * adamping
    aleft, aright	pan2 asignal, p7
    ; Stereo audio output to be routed in the orchestra header.
    		outleta "leftout", aleft
    		outleta "rightout", aright
    endin

    instr Reverberator
    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    ; Stereo input.
    aleftin 	inleta "leftin"
    arightin 	inleta "rightin"
    idelay 		= p4
    icutoff 	= p5
    aleft, aright 	reverbsc aleftin, arightin, idelay, icutoff
    ; Stereo output.
    		outleta "leftout", aleft
    		outleta "rightout", aright
    endin

    instr Compressor
    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    ; Stereo input.
    aleftin 	inleta "leftin"
    arightin 	inleta "rightin"
    kthreshold 	= 25000
    icomp1 		= 0.5
    icomp2 		= 0.763
    irtime 		= 0.1
    iftime 		= 0.1
    aleftout 	dam aleftin, kthreshold, icomp1, icomp2, irtime, iftime
    arightout 	dam arightin, kthreshold, icomp1, icomp2, irtime, iftime
    ; Stereo output.
    		outleta "leftout", aleftout
    		outleta "rightout", arightout
    endin

    instr Soundfile
    ;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
    ; Stereo input.
    aleftin 	inleta "leftin"
    arightin 	inleta "rightin"
    		outs aleftin, arightin
    endin

    </CsInstruments>
    <CsScore>

    ; It is not necessary to activate "effects" or create f-tables in the score!
    ; Overlapping notes create new instances of instruments with proper connections.

    i "SimpleSine" 1 5 60 85
    i "SimpleSine" 2 5 64 80
    i "Moogy" 3 5 67 75
    i "Moogy" 4 5 71 70
    ;1 extra second after the performance
    e 1

    </CsScore>
    </CsoundSynthesizer>

## See Also

outleta outletk outletkid outletf inletk inletkid inletf connect alwayson ftgenonce

More information on this opcode: http://www.csoundjournal.com/issue13/signalFlowGraphOpcodes.html , written by Michael Gogins

## Credits

By: Michael Gogins 2009

Prev | Up | Next
initc7 | Home | inletk