STKBlowBotl
Prev | Orchestra Opcodes and Operators | Next

## STKBlowBotl

STKBlowBotl — STKBlowBotl uses a helmholtz resonator (biquad filter) with a polynomial jet excitation.

## Description

Plugin opcode in stkopd.

This opcode implements a helmholtz resonator (biquad filter) with a polynomial jet excitation (a la Cook).

## Syntax

    asignal STKBlowBotl ifrequency, iamplitude, [knoise, kv1[, klfo, kv2[, klfodepth, kv3[, kvol, kv4]]]]

## Initialization

ifrequency -- Frequency of note played, in Hertz.

iamplitude -- Amplitude of note played (range 0-1).

## Performance

knoise -- controller 4, gain of noise. Value range of kv1 is 0-127.

klfo -- controller 11, speed of low-frequency oscillator. Value range of kv2 is 0-127.

klfodepth -- controller 1, depth of low-frequency oscillator. Value range of kv3 is 0-127.

kvol -- controller 128, volume. Value range of kv4 is 0-127.

| Notes
The code for this opcode is taken directly from the BlowBotl class in the Synthesis Toolkit in C++ by Perry R. Cook and Gary P. Scavone. More on the STK classes can be found here: https://ccrma.stanford.edu/software/stk/classes.html kc1, kv1, kc2, kv2, kc3, kv3, kc4, kv4, kc5, kv5, kc6, kv6, kc7, kv7, kc8, kv8 -- Up to 8 optional k-rate controller pairs for the STK opcodes. Each controller pair consists of a controller number (kc) followed by a controller value (kv). Both the controller numbers and the controller values are krate variables. However, during a performance, normally the controller numbers stay fixed while the corresponding controller values may change at any time. The order of the controller pair is arbitrary, as long as they are after iamplitude. Also, it is not needed that all controller pairs are used.

## Examples

Here is an example of the STKBlowBotl opcode. It uses the file STKBlowBotl.csd.

Example 1001. Example of the STKBlowBotl opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o STKBlowBotl.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    ipch	= p4
    kv1	line p5, p3, p6					;gain of noise
    kv4	line	100, p3, 70				;volume

    asig	STKBlowBotl cpspch(ipch), 1, 4, kv1, 11, 10, 1, 50, 128, kv4
    asig	=	asig * .5				;too loud
    	outs	asig, asig
    endin

    </CsInstruments>
    <CsScore>

    i 1 0 2 9.00 20 100
    i 1 + 5 8.03 120 0
    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Michael Gogins (after Perry Cook)
Irreducible Productions
New York, NY

New in Csound version 5.11

Prev | Up | Next
STKBeeThree | Home | STKBlowHole